**PUTSI Beta Test Issues**

**Hardware**

* 78L33 when powering CPU runs hot
* Digital input circuit divides pull-up voltage down to about 1V. Can be raised by reducing 22K resistor or increasing

**Software (see Release notes in documentation)**

* Config mode not working correctly. Flags are all being set to zero after programming.
  + Test put in to enter config mode if WiFi or USB are not enabled.
* Ports removed from setup, not likely to change, and can be reenabled in firmware.
* Auto Config enable removed from set, now enabled with Wi-Fi mode automatically.